# $Id: run.def 1403 2010-07-01 09:02:53Z fairhead $
#
## Fichier de configuration general
## 
INCLUDEDEF=physiq.def
INCLUDEDEF=config.def
INCLUDEDEF=traceur.def
INCLUDEDEF=run_icosa.def
INCLUDEDEF=earth_const.def
INCLUDEDEF=vert.def

## Type de calendrier utilise
## valeur possible: earth_360d (defaut), earth_365d, earth_366d
calend=_AUTOBLOCKER_
## Jour de l'etat initial ( = 350  si 20 Decembre ,par expl. ,comme ici )
dayref=_AUTOBLOCKER_
##  Annee de l'etat  initial (   avec  4  chiffres   )
anneeref=_AUTOBLOCKER_

## Remise a zero de la date initiale
raz_date=_AUTOBLOCKER_

## niveau d'impression de controle
prt_level=0

###
### Informations sur la configuration utilisee
###
### type_ocean = force / slab  /couple
### type_ocean is modified automatically by the lmdz.driver
type_ocean= force
### version_ocean = nemo / opa8
version_ocean=nemo
### activation passage courants surface ocean-glace
cpl_current=y
### VEGET= y si ORCHIDEE, =n si bucket
### VEGET is modified automatically by the lmdz.driver
VEGET= n
### To activate XIOS ouputs only, set n to use IOIPSL
ok_all_xml= y
### Only read by ce0l : Do not set land points on Antartic
no_ter_antartique=y
### Do not call phytrac to speed things up
iflag_phytrac=0

