# $Id$
#
INCLUDEDEF=orchidee.def
INCLUDEDEF=orchidee_pft.def

# Parameters of the driver differ between the coupled and off-line configs
#**************************************************************************
# Time length for one intergration 
# (default full lenght of forcing file)
TIME_LENGTH = _AUTO_

# Time in the forcing file at which the model start if start date is
# not set by the forcing file 
# (default 0)
TIME_SKIP = _AUTO_

# Time length for one intergration (default full lenght of forcing file)
START_DATE = _AUTO_
END_DATE = _AUTO_ 
DT_SECHIBA = 1200
FORCING_FILE = forcing_yearm1.nc forcing_year.nc forcing_yearp1.nc


# If DRIVER_reset_time=y, read the year from forcing file instead of
# taking it from restart file (default n)
DRIVER_reset_time = _AUTO_

# Name of restart file for the driver (default NONE)
RESTART_FILEIN = _AUTOBLOCKER_

# Value for atmospheric CO2 could be interactive (LMDz), a time series or fixed
# (default=350)
# ATM_CO2=287.14 : Year 1860 specified for TRENDY2 spinup
ATM_CO2 = _AUTO_: DEFAULT = 287.14

# Domain description 
#**************************************************************************
GRID_FILE = NONE

# To limit regional domain, full size of the forcing file or global domain is default
#WEST_EAST = -180.0, 180.0
#SOUTH_NORTH = -90.0, 90.0
#WEST_EAST = -19.7, 62.7
#SOUTH_NORTH = -6.7, 62.7

# Time period over which to distribute the precipitation 
#**************************************************************************
# In the driver files precipitation is the accumulated value over the
# time step of the driver file (e.g. 6 hours). In ORCHIDEE it needs to
# be decided whether over which time period (in seconds) this precip will come
# down. Short periods make rain storms, long periods make drizzel.
SPRED_PREC_SEC = 3600



